Introduction

Name：ZL-2201 Safety shoes impact tester

Description

safety shoes impact tester,safety footwear impact tester

Introduce:

This machine is installed a steel striker adaptered to fall freely on vertical guides from

a predetermined height to give the required impact energy to the toe of safety footwear for measuring

the degree of the dent. In addition, the toecap should not develop any cracks on the test axis with go through the material.

Standard:

It complies with BS-953, EN-344, ANSI-41, CSA-Z195, ISO 8782

Technology Parameters:

Striker Weight	(EN) 20±0.2kg, (BS, ANSI) 22.7KG
Drop Height	0~1100mm auto adjustable
Impact Energy	(EN)200J, (BS, ANSI)1002J
Striker	(EN)3±0.1mm, (ANSI)ø25.4
Dimension	70×70×180cm
Weight	185kg
Power	AC220V/50Hz or others