Introduction

Name：ZL-2202 Safety shoes Puncture Resistance tester

Safety shoe puncture resistance tester

Safety Shoe Puncture Resistance Tester is used to measures the compression strength for safety shoes steel head and

puncture-resistant performance for steel plate.

It Suitable for all types of steel head compression for safety shoes and puncture-resistant test for steel plate, and to

prevent the injury of accident to operators in the workplace by wearing owing to the security of shoes.

Specification:

sensor capacity	20KN , 15±0.1KN
load resolution	1/20000
Accuracy	within 1%
Press plate hardness	60HRC
Puncture steel nail	Diameter :4.5±0.05）mm, hardness:60HRC
display system	English controller
Test speed	5-500 mm/min, the speed can be adjustable

Compression speed: （5±2）mm/min

Puncture speed:（10±3）mm/min
Stroke display	0.01mm
Unit	Kg, N. LB can be changed each other
Motor	AC motor+ reducer
Measuring fixture	compression/puncture fixture
dimension	82*58*71cm
weight	148kg
Power	AC220V 50HZ 0.4KW

Standard:

GB 21146-2007;GB 21147-2007、GB 21148-2007 ,GB/T 20991-2007