Introduction

Name：ZL-2207 safety shoe anti-static tester

Use:

It's suitable for testing resistance of complete shoes or shoe material,to realize sample static disperse effect.

Test standards:SATRA—TM240,EN-344,GB/T 4386,ANSI Z41,ISO20345,ISO08782,GB/T20991,GB4385

Specification:

Test range:0.001MΩ-20GΩ(1×103 ~2×1013Ω)

Test accuracy:±2%/±5%/±10%

Outside size:14.9*8.6*2.4cm

Internal voltage:50V,100V

Standard configuration:5mm stainless steel ball 4kg